{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["BIAS_TGA2237-SM"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"BIAS_TGA2237-SM","index":0,"n_rows":12,"n_cols":7,"rows_kept":12,"cut":false,"hidden":false,"merged":[]}
["Comment","Description","Designator","Footprint","LibRef","Quantity"]
["47 мкФ","планарный конденсатор","C1, C5, C6","C1206","C1206",3,"https://www.chipdip.ru/product0/8011896482"]
["10 мкФ","планарный конденсатор","C2","C1206","C1206",1,"https://www.chipdip.ru/product0/9000067594"]
["0,1 мкФ","планарный конденсатор","C3, C4, C7, C8, C9, C10","C0603","C0603",6,"https://www.chipdip.ru/product0/8032641374"]
["LM2662MX_NOPB","Charge pump","DA1","SOIC127P600X175-8N","LM2662MX_NOPB",1,"https://www.chipdip.ru/product/lm2662m-nopb-ti"]
["TL072CDT","Операционный усилитель, двухканальный, 13 В, 4 МГц","DA2","SOIC127P600X175-8N","TL072CDT",1,"https://www.chipdip.ru/product/tl072cdt?from=suggest_product"]
["SN74LVC1G14DBV","szhmit trigger","DD1","DBV_SOT-23-5","SN74LVC1G14DBV",1,"https://www.chipdip.ru/product/sn74lvc1g14dbvr-umw"]
["10кОм","планарный резистор","R1","R0603","R0603",1,"https://www.chipdip.ru/product/0.1w-0603-10-kom-5"]
["0 Ом","планарный резистор","R2, R3, R5","R0603","R0603",3,"https://www.chipdip.ru/product/0.1w-0603-0-om-5"]
["1кОм","планарный резистор","R4, R6, R7","R0603","R0603",3,"https://www.chipdip.ru/product0/8007154148"]
["10кОм","подстроечный резистор","RP1, RP2","3224W","3224W",2,"https://www.chipdip.ru/product0/8027756517"]
["PLS-2","PLS-2","XP1, XP2, XP3, XP4","PLS-2","PLS-2",4,"https://www.chipdip.ru/product/pls-40"]